FM2M D-Clock 1.2 for EdgeTX
============================

Requirements
------------
* EdgeTX 2.11 or newer
* Radio with a 480x272 color LCD

D-Clock 1.2 is designed for the 480x272 full-screen layout. The widget may
start on radios with other screen resolutions, but its layout will be
incorrect or elements may appear shronked or outside the visible area.

Installation
------------
1. Unpack fm2m-dclock-120-edgetx.zip.
2. Copy the WIDGETS folder to the root of the radio SD card.
3. Merge folders and replace application files when prompted.
4. Add "FM2M D-Clock" to a full-screen telemetry layout.

User settings are stored in:

  /WIDGETS/FM2MDC/USER/dclock.cfg

The package does not contain this file, so updating the widget preserves
existing settings.

Information and community
-------------------------
FM2M website:
https://fm2m.online

FM2M Discord:
https://discord.gg/uSfMKWNkjT

Happy flying to the moon
Robert
